#
DIAGNOSTIC MONITORING TEST RESULTS [L3]

BME010200000W11
• The purpose of this test mode is to confirm the result of the OBD monitor diagnostic test results. The result values stored when a particular monitored item is completed are displayed. If the monitored item is not completed, initial value is displayed.

TEST ID | Description | Related system
--- | --- | ---
10:01:0A | Rich to lean sensor threshold voltage | HO2S
10:02:0A | Lean to rich sensor threshold voltage
10:03:0A | Low sensor voltage for switching time calculation
10:04:0A | High sensor voltage for switching time calculation
10:05:10 | Rich to lean sensor switching time
10:06:10 | Lean to rich sensor switching time
10:0A:10 | Sensor period
10:80:20 | Front and Rear HO2S switching time ratio | TWC