#
REAR PILLAR (OUTER) AND CORNER PLATE REMOVAL

BME098070442B01
• The rear fender panel and rear end panel are removed.
When replacing the rear pillar outer and corner plate at the same time.
• Drill weld locations marked (A), (B), (C) and (E) and remove from the outside.
When replacing the corner plate and corner junction at the same time.
• Drill weld locations marked (B), (C) and (D) and remove from the outside.