#
FUEL PUMP UNIT REMOVAL/INSTALLATION [L3]

BME011413350W01

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, do not damage the sealing surface of the fuel pump unit when removing or installing.

  Caution

  • Disconnecting/connecting the quick release connector without cleaning it may possibly cause damage to the fuel pipe and quick release connector. Always clean the quick release connector joint area before disconnecting/connecting using a cloth or soft brush, and make sure that it is free of foreign material.

1. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [L3].)

2. Disconnect the negative battery cable.

3. Remove the front seats.

4. Remove the front scuff plates.

5. Remove the rear scuff plates.

6. Remove the console lower cover.

7. Loosen the parking brake lever installation bolts.

8. Partially peel back the floor covering until the service hole cover appears.

9. Remove in the order indicated in the table.

1 | Service hole cover
2 | Connector
3 | Plastic fuel hose (See Plastic Fuel Hose Removal Note) (See Plastic Fuel Hose Installation Note)
4 | Fuel pump unit

10. Install in the reverse order of removal.

11. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [L3].)

## Plastic Fuel Hose Removal Note

  Caution

  • The quick release connector may be damaged if the tab is bent excessively. Do not expand the tab over the stopper.

1. Disconnect the quick release connector.

  (1) Push the tab on the locking coupler 90 degrees until it stops.
  (2) Pull the fuel hose straight back.

  Note

  • The stopper may be removed from the quick connector. Take care not to lose it.
  Reinstall it to the quick release connector before reconnecting the fuel line.
  • The locking coupler has two internal locking tabs which retain the fuel pipe. Be sure that the tab on the locking coupler is rotated until it stops to release two internal locking tabs.

2. Cover the disconnected quick release connector and fuel pipe with vinyl sheets or the like to prevent them from being scratched or contaminated with foreign material.

## Plastic Fuel Hose Installation Note

  Note

  • A checker tab is integrated with quick release connector for new plastic fuel hoses. The checker tab will be released from the quick release connector after it is completely engaged with the fuel pipe.

1. When the retainer is not removed, perform the following procedure.

  (1) Inspect the fuel pump unit sealing surface for damage and deformation, and replace as necessary.

  • If the quick release connector O-ring is damaged, replace the plastic fuel hose.

  (2) Slightly apply clean engine oil to the sealing surface of the fuel pump unit.
  (3) Align the fuel pipe on the fuel pump unit and quick release connector so that the tabs of the retainer are correctly fitted into the quick release connector. Push the quick release connector straight into the retainer until a click is heard.
  (4) Lightly pull and push the quick release connector a few times by hand and verify that it can move 2.0-3.0 mm {0.08-0.11 in} and it is connected securely.

  • If quick release connector does not move at all, verify that O-ring is not damaged and slipped, and reconnect the quick release connector.

2. When the retainer is removed, perform the following procedure.