#
PRE-DELIVERY INSPECTION

BME000000000W11

## Pre-Delivery Inspection Table

### Exterior

INSPECT and ADJUST, if necessary, the following items to specification:

□Glass, exterior bright metal and paint for damage

□Wheel lug nuts

□All weatherstrips for damage or detachment

□Tire pressures

□Headlight cleaner and fluid level (if equipped)

□Operation of bonnet release and lock

□Operation of trunk lid and fuel-filler lid opener

□Door operation and alignment including side door and back door

□Headlight aiming

INSTALL the following parts:

□Flap (front)

□Wheel caps or rings (if equipped)

### Under bonnet-engine off

INSPECT and ADJUST, if necessary, the following items to specification:

□Fuel, engine coolant, and hydraulic lines, fittings, connections, and components for leaks

□Engine oil level

□Brake and clutch fluid level

□Windshield washer reservoir fluid level

□Manual transmission/Transaxle oil level

□Radiator coolant level and specific gravity

□Tightness of water hose clamps

□Tightness of battery terminals, electrolyte level and specific gravity

□Differential oil level

### Interior

INSTALL the following items:

□Fuse for accessories

INSPECT the operations of the following items:

□Seat controls (slide and recline) and headrests

□Folding rear seat

□Door locks, including childproof door locks

□Seat belts and warning system

□Ignition switch and steering lock

□Transmission/Transaxle range switch

□Warning buzzers

□Ignition key reminder alarm

□Air bag system using warning light

□Cruise control system (if equipped)

□Power door lock

□Shift-lock system (if equipped)

□Starter interlock

□All lights including warning, and indicator lights

□Horn, wipers, and washers

□Wiper blades performance

Clean wiper blades and windshield, if necessary

□Antenna

□Audio system

□Cigarette lighter and clock

□Power windows (if equipped)

□Heater, defroster, and air conditioner at various mode selections (if equipped)

INSPECT the following items:

□Presence of spare fuse

□Upholstery and interior finish

INSPECT and ADJUST, if necessary, the following items:

□Operation and fit of windows

□Pedal height and free play of clutch pedal

□Parking brake

### Under bonnet-engine running at operating temperature

INSPECT the following items:

□Automatic transmission/Transaxle fluid level

□Operation of idle-up system for electrical load, air conditioner or power steering (if equipped)

□Ignition timing

□Idle speed

□Operation of throttle position sensor

### On hoist

INSPECT the following items:

□Manual transmission/Transaxle oil level

□Underside fuel, coolant and hydraulic lines, fittings, connections, and components for leaks

□Tires for cuts or bruises

□Steering linkage, suspension, exhaust system, and all underside hardware for looseness or damage

### Road test

INSPECT the following items:

□Brake operation

□Clutch operation

□Steering control

□Operation of gauges

□Squeaks, rattles, and unusual noises

□Engine general performance

□Emergency locking retractors and automatic locking retractors

□Cruise control system (if equipped)

□Operation of meters and gauges, squeaks, rattles, and abnormal noises

### After road test

INSPECT for necessary owner information materials, tools, and spare tire in vehicle

The following items must be completed just before delivery to your customer.

□Load test battery and charge if necessary (Load test result: Volts)

□Adjust tire pressure to specification (Specified tire pressure is indicated on the door label.)

□Clean outside of vehicle

□Install fuses for accessories

□Remove seat and cabin carpet protective covers

□Vacuum inside of vehicle