#
GLASS PANEL ADJUSTMENT

BME091569810202

1. Fully close the glass panel.

2. Measure the gap and height between the glass panel and body.

3. If not as specified, loosen the glass panel installation screws and reposition the glass panel.

Clearance

  a: 0.2-2.2 mm {0.008-0.086 in}
  b: 0 mm {0 in}

4. Tighten the installation screws.

5. Insert a prepaid card between the weatherstrip and the body of the vehicle. Verify that the sunroof is shut tightly (there is resistance when the prepaid card is moved).

  • If the sunroof is not shut tightly, readjust by performing Steps 3 and 4.