#
NO.25 ENGINE STALLS WHEN DRIVING AT SLOW SPEED OR STOPPING [JA5A-EL]

BME050301030261

25 | Engine stalls when driving at slow speeds or stopping
DESCRIPTION | • Engine stalls when the brake pedal is depressed while driving at low speed or stopping.
POSSIBLE CAUSE | • The malfunction is on engine control side (e.g. Fuel injection control, IAC system)

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Go to No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See NO.10 LOW IDLE/STALLS DURING DECELERATION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
Is the engine control system normal?
Yes
Go to No.24 "ENGINE STALLS WHEN SHIFTED TO D, S, L RANGES, OR IN R POSITION".
No | Repair or replace any malfunctioning parts according to the inspection results.
2 | • Verify the test results.

  - If normal, return to the diagnostic index to service any additional symptoms.
  - If the malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform repair or diagnosis.

  • If the vehicle is repaired, troubleshooting is completed.
  • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.