#
DTC P0341 [MZR-CD (RF Turbo)]

BME010200300W10

DTC P0341 | CMP sensor circuit performance problem
--- | ---
DETECTION CONDITION | • PCM monitors input signal from CMP sensor while engine is running. If input signal from CMP sensor is not proper pulse number, PCM determines CMP sensor circuit performance problem.
POSSIBLE CAUSE | • CMP sensor malfunction • Connector or terminal malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
2 | VERIFY DTC P0341 DETECTED AGAIN • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Go to next step.
No | Intermittent concern exists. Go to "Intermittent Concern Troubleshooting". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
3 | INSPECT POOR CONNECTION OF CMP SENSOR CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to Step 6.
No | Go to next step.
4 | INSPECT CMP SENSOR • Inspect CMP sensor. (See CAMSHAFT POSITION (CMP) SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace CMP sensor, go to Step 6. (See CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
5 | INSPECT POOR CONNECTION OF PCM CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to next step.
No | Go to next step.
6 | VERIFY TROUBLESHOOTING OF DTC P0341 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Replace PCM, go to next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Is there any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.