#
FUEL-FILLER LID AND OPENER REMOVAL/INSTALLATION

BME091456890201

1. To remove the fuel-filler lid opener, remove the left side trunk side trim.

2. To remove the fuel-filler lid opener cable, perform the following and turn over the front floor covering.

  (1) Remove the driver-side front seat.
  (2) Remove the driver-side front scuff plate.
  (3) Remove the driver-side rear scuff plate.
  (4) Remove the driver-side B-pillar lower trim.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Adjust the fuel-filler lid. (See FUEL-FILLER LID ADJUSTMENT.)

L.H.D.

R.H.D.

1 | Fuel-filler lid
2 | Sliding door stopper cable
3 | Nut
4 | Fuel-filler lid opener
5 | Fuel-filler lid opener lever
6 | Fuel-filler lid opener cable