#
DTC 07 ERR01 OR 07:ER01

BME090266900W23

DTC 07 ERR01 or 07:Er01 | MD player
DETECTION CONDITION | • MD player cannot implement insert and eject commands.
POSSIBLE CAUSE | • Defective MD (broken or foreign material stuck/attached) • MD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is MD able to be ejected? | Yes | Go to next step.
No | Replace MD player.
2 | INSPECT MD • Inspect condition of MD where error has occurred. • Is MD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace MD, then go to next step.
3 | INSPECT MD PLAYER • Clear DTC. • Insert and eject MD with no defect. • Start on-board diagnostic test mode. • Is DTC 07 ERR01 or 07:Er01 displayed? | Yes | Replace MD player.
No | Troubleshooting completed.