#
THERMOSTAT REMOVAL/INSTALLATION [AJ]

BME011215171202

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [L3, AJ].)

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [AJ].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [AJ].)

1 | Upper radiator hose
2 | Lower radiator hose
3 | Thermostat cover
4 | O-ring
5 | Thermostat (See Thermostat Installation Note.)

## Thermostat Installation Note

1. Install the thermostat into the thermostat case with the jiggle pin at the top.