#
POWER BRAKE UNIT REMOVAL/INSTALLATION

BME041143800W02

1. For the L.H.D. model, remove the battery.

2. For the L.H.D. model, remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. For the L.H.D. model (MZR-CD (RF Turbo)), remove the brake pipes between the master cylinder and brake pipe joint.

4. Remove the master cylinder. (See MASTER CYLINDER REMOVAL/INSTALLATION.)

5. For the MZR-CD (RF Turbo) model, remove the vacuum switch. (See VACUUM SWITCH REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

6. Remove in the order indicated in the table.

1 | Vacuum hose
2 | Snap pin
3 | Clevis pin
4 | Nut
5 | Fork
6 | Nut
7 | Power brake unit
8 | Gasket
9 | Spacer
10 | Gasket

7. Install in the reverse order of removal.