#
BASE REMOVAL

BME091269240201

  Warning

  • Using a SST (piano wire) with bare hands can cause injury. Always wear gloves when using a SST (piano wire).

1. Remove the rearview mirror.

2. Wind each end of a wire around a bar.

  Note

  • Use a long sawing action to spread the work over the whole length of the SST (piano wire) to prevent it from breaking.

3. Saw through the sealant to remove the base.