#
CONTROL VALVE BODY INSTALLATION [FN4A-EL]

BME051721100202

## On-Vehicle Installation

  Caution

  • Be sure to align the parking rod with the manual valve.

1. Install the accumulator springs and accumulators into the transaxle case.

Spring | Outer diameter (mm {in}) | Free Length (mm {in}) | No. of coils | Wire diameter (mm {in})
--- | --- | --- | --- | ---
Servo apply accumulator large spring | 21.0 {0.827} | 67.8 {2.669} | 10.3 | 3.5 {0.138}
Servo apply accumulator small spring | 13.0 {0.512} | 67.8 {2.669} | 17.1 | 2.2 {0.087}
Forward accumulator small spring | 21.0 {0.827} | 75.0 {2.953} | 10.7 | 2.3 {0.091}
Forward accumulator large spring | 15.6 {0.614} | 49.0 {1.929} | 7.7 | 2.4 {0.094}

2. Install the control valve body component.

Tightening torque

  7.8-10.8 N·m
  {80-110 kgf·cm, 70-95 in·lbf}

Bolt length (measured from below the head)

  Mark B: 40 mm {1.575 in}
  No mark: 70 mm {2.756 in}

3. Install the oil strainer.

4. Match the wiring harness colors, then connect the solenoid connectors and ground, and install the TFT sensor.

Spring | Color of connector (harness side)
--- | ---
Pressure control solenoid | Black
Shift solenoid A | White
Shift solenoid B | Blue
Shift solenoid C | Green
Shift solenoid D | White
Shift solenoid E | Black

5. Apply a light coat of silicon sealant to the contact surfaces of the oil pan and transaxle case.

6. Install the oil pan.

Tightening torque

  6-8 N·m {62-81 kgf·cm, 53-70 in·lbf}

7. Connect the negative battery cable.

8. Add ATF and with the engine idling, inspect the ATF level. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FN4A-EL].)

9. Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [FN4A-EL].)

10. Perform the road test. (See ROAD TEST [FN4A-EL].)