#
CONTROL SYSTEM WIRING DIAGRAM [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed))

BME014000000T82

## With Immobilizer System

1 | Battery
2 | Main fuse
3 | Starter
4 | Generator
5 | Ignition switch
6 | DLC
7 | To ABS/TCS HU/CM
8 | Instrument cluster
9 | Main relay
10 | Fuel pump relay
11 | Fuel pump unit
12 | PSP switch
13 | HO2S (front, RH) (integrated with HO2S heater)
14 | HO2S (front, LH) (integrated with HO2S heater)
15 | HO2S (rear, RH) (integrated with HO2S heater)
16 | HO2S (rear, LH) (integrated with HO2S heater)
17 | EGR valve
18 | MAF/IAT sensor
19 | DLC-2
20 | Generator warning light
21 | MIL
22 | Front blower motor
23 | PCM
24 | A/C relay
25 | A/C switch
26 | A/C amplifier
27 | Refrigerant pressure switch (low and high pressure)
28 | Refrigerant pressure switch (middle pressure)
29 | A/C compressor
30 | Cooling fan relay
31 | Main fan motor
32 | Fan control module
33 | Fan switch
34 | Additional fan motor
35 | Front resister
36 | IAC valve
37 | Purge solenoid valve
38 | ECT sensor
39 | TP sensor
40 | EGR boost sensor
41 | EGR boost sensor solenoid valve
42 | IMCC actuator
43 | CMP sensor
44 | CKP sensor
45 | Fuel injector No.1
46 | Fuel injector No.2
47 | Fuel injector No.3
48 | Fuel injector No.4
49 | Fuel injector No.5
50 | Fuel injector No.6
51 | Capacitor
52 | Ignition coil No.1
53 | Ignition coil No.2
54 | Ignition coil No.3
55 | Ignition coil No.4
56 | Ignition coil No.5
57 | Ignition coil No.6
58 | Brake light
59 | Brake switch
60 | Cruise CM
61 | KS
62 | To battery
63 | To instrument cluster
64 | With A/C
65 | Without A/C
66 | With HO2S (rear)
67 | Immobilizer unit
68 | Front blower motor relay
69 | To IG1
70 | To TCM
71 | To main relay terminal A
72 | To PCM terminal 5
73 | To PCM terminal 30
74 | To PCM terminal 46
75 | To PCM terminal 47
76 | To PCM terminal 69
77 | To PCM terminal 72
78 | To PCM terminal 73
79 | To PCM terminal 98
80 | To PCM terminal 99
81 | To EGR valve
82 | To A/C system
83 | To fan control module
84 | Except for China or without rear HO2S for Australian, General (R.H.D.) specs.
85 | China or without rear HO2S for Australian, General (R.H.D.) specs.

## Without Immobilizer System

1 | Battery
2 | Main fuse
3 | Starter
4 | Generator
5 | Ignition switch
6 | DLC
7 | To ABS/TCS HU/CM
8 | Instrument cluster
9 | Main relay
10 | Fuel pump relay
11 | Fuel pump unit
12 | PSP switch
13 | HO2S (front, RH) (integrated with HO2S heater)
14 | HO2S (front, LH) (integrated with HO2S heater)
15 | HO2S (rear, RH) (integrated with HO2S heater)
16 | HO2S (rear, LH) (integrated with HO2S heater)
17 | EGR valve
18 | MAF/IAT sensor
19 | DLC-2
20 | Generator warning light
21 | MIL
22 | Front blower motor
23 | PCM
24 | A/C relay
25 | A/C switch
26 | A/C amplifier
27 | Refrigerant pressure switch (low and high pressure)
28 | Refrigerant pressure switch (middle pressure)
29 | A/C compressor
30 | Cooling fan relay
31 | Main fan motor
32 | Fan control module
33 | Fan switch
34 | Additional fan motor
35 | Front resister
36 | IAC valve
37 | Purge solenoid valve
38 | ECT sensor
39 | TP sensor
40 | EGR boost sensor
41 | EGR boost sensor solenoid valve
42 | IMCC actuator
43 | CMP sensor
44 | CKP sensor
45 | Fuel injector No.1
46 | Fuel injector No.2
47 | Fuel injector No.3
48 | Fuel injector No.4
49 | Fuel injector No.5
50 | Fuel injector No.6
51 | Capacitor
52 | Ignition coil No.1
53 | Ignition coil No.2
54 | Ignition coil No.3
55 | Ignition coil No.4
56 | Ignition coil No.5
57 | Ignition coil No.6
58 | Brake light
59 | Brake switch
60 | Cruise CM
61 | KS
62 | To battery
63 | To instrument cluster
64 | With A/C
65 | Without A/C
66 | With HO2S (rear)
67 | To fan control module
68 | Front blower motor relay
69 | To IG1
70 | To TCM
71 | To main relay terminal A
72 | To PCM terminal 5
73 | To PCM terminal 30
74 | To PCM terminal 46
75 | To PCM terminal 47
76 | To PCM terminal 69
77 | To PCM terminal 72
78 | To PCM terminal 73
79 | To PCM terminal 98
80 | To PCM terminal 99
81 | To EGR valve
82 | To A/C system
83 | Except for China or without rear HO2S for Australian, General (R.H.D.) specs.
84 | China or without rear HO2S for Australian, General (R.H.D.) specs.