#
A/C CUT-OFF CONTROL OPERATION [AJ]

BME014000000T74

A/C cut condition | A/C stop time | Purpose
--- | --- | ---
During cranking | For approx. 4 s | Stability improvement
Vehicle start off | For approx. 3 s | Acceleration performance improvement
Acceleration (throttle valve opening angle above 50%) | For approx. 5 s
ECT is approx. 113 °C {235 °F} | Alternates between 10 s ON and 10 s OFF until ECT falls below 107 °C {224 °F} | Engine reliability improvement
ECT is above 117 °C {242 °F} | Until ECT falls below 110 °C {230 °F}
Engine speed below 1,500 rpm and PSP switch ON | For approx. 1 s | Engine stability at idle improvement