#
SEDIMENTOR WATER DRAINING [MZR-CD (RF Turbo)]

BME011420490W04

1. Disconnect the negative battery cable.

2. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

3. Loosen the drain plug located at the bottom of the fuel filter.

4. Pump the priming pump and drain the water.

5. After all the water has been drained, tighten the drain plug.

6. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

7. Reconnect the negative battery cable.