#
THERMOSTAT INSPECTION

BME011215171W04

1. Inspect the thermostat for the following.

  • Closed valve in room temperature
  • Opening temperature and lift of the valve
  - If there is any malfunction, replace the thermostat.

Condition | Specification
--- | ---
L3 | MZR-CD (RF-Turbo)
Initial-opening temperature | (°C {°F}) | 80-84 {176-183} | 80-84 {176-183}
Full-open temperature | (°C {°F}) | 97 {207} | 95 {203}
Full-open lift | (mm {in}) | More than 8.0 {0.31} | More than 8.5 {0.33}