#
FRONT FRAME (REAR) REMOVAL

BME098053390B01

1. The sections marked (A), (B) and (C) are the same, only the viewing angles are different.

2. It is not necessary to drill the 2 weld locations marked (D). (These sections are connections of the frame (rear) and frame reinforcement, and are replaced at the same time.)

3. As drilled the 4 weld locations marked (E) cannot be checked from underneath, check from the room.