#
SECONDARY SHAFT COMPONENTS DISASSEMBLY

BME051517301M02

1. Disassemble in the order indicated in the table.

1 | Secondary shaft rear bearing adjust shim
2 | Snap ring
3 | Snap ring
4 | C ring holder
5 | Secondary shaft C ring
6 | Secondary shaft rear bearing (See Secondary Shaft Rear Bearing Disassembly Note.)
7 | Snap ring
8 | 5th gear (See 4th Gear and 5th Gear Disassembly Note.)
9 | 4th gear
10 | 4th gear adjustment shim
11 | 3rd/4th secondary shaft spacer
12 | 3rd gear (See 3rd Gear, 2nd Gear, 2nd Needle Bearing, 2nd Bushing, 2nd Inner Synchronizer Component, 1st/2nd Clutch Hub Set, 1st Inner Synchronizer Component, 1st Needle Bearing, 1st Bushing, 1st Gear and Reverse Main Gear Disassembly Note.)
13 | 2nd gear
14 | 2nd needle bearing
15 | 2nd bushing
16 | 2nd inner synchronizer component
17 | 1st/2nd clutch hub set
18 | 1st inner synchronizer component
19 | 1st needle bearing
20 | 1st bushing
21 | 1st gear
22 | Reverse main gear
23 | Secondary shaft
24 | Synchronizer key spring
25 | 1st/2nd synchronizer key
26 | 1st/2nd clutch hub and sleeve

## Secondary Shaft Rear Bearing Disassembly Note

1. Remove the secondary shaft rear bearing using the SSTs.

## 4th Gear and 5th Gear Disassembly Note

1. Remove the 4th gear and 5th gear at the same time using the SSTs.

## 3rd Gear, 2nd Gear, 2nd Needle Bearing, 2nd Bushing, 2nd Inner Synchronizer Component, 1st/2nd Clutch Hub Set, 1st Inner Synchronizer Component, 1st Needle Bearing, 1st Bushing, 1st Gear and Reverse Main Gear Disassembly Note

1. Remove the 3rd gear, 2nd gear, 2nd needle bearing, 2nd bushing, 2nd inner synchronizer component, 1st/2nd clutch hub set, 1st inner synchronizer component, 1st needle bearing, 1st bushing, 1st gear and reverse main gear at the same time using the SST.