#
COOLING FAN MOTOR REMOVAL/INSTALLATION [L3]

BME011215025202

1. Disconnect the negative battery cable.

2. Remove the transverse member. (See TRANSVERSE MEMBER REMOVAL/INSTALLATION.)

3. Remove the engine mount member.

4. Remove the No.2 engine mount.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

1 | Fan control module connectors
2 | Radiator cowling
3 | Main fan
4 | Additional fan
5 | Main fan motor
6 | Additional fan motor
7 | Fan control module