#
SUNROOF UNIT REMOVAL/INSTALLATION

BME091569850W01

1. Disconnect the negative battery cable.

2. Remove the headliner.

3. Remove the glass panel.

4. Disconnect the front and rear drain hose from the sunroof frame.

5. Remove the roof harness from the sunroof frame.

6. Remove the bolts and nuts, and then remove the sunroof unit.

7. Install in the reverse order of removal.

8. Adjust the glass panel. (See GLASS PANEL ADJUSTMENT.)