#
AIR FILTER REMOVAL/INSTALLATION

BME071161140203

## TYPE A

  Caution

  • The air filter is made of static electric fibers. If the filter is removed and exposed to air for a long time, dirt and dust will collect on the fibers, rendering the filter unusable. After removing the air filter, store it in a plastic bag.

1. Remove the glove compartment.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Cover
2 | Air filter

## TYPE B

1. Remove the glove compartment.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Cover
2 | Air filter (1)
3 | Air filter (2)