#
LOWER MODULE REMOVAL/INSTALLATION

BME092066900204

1. Disconnect the negative battery cable.

2. Remove the audio unit.

3. Remove in the order indicated in the table.

1 | Cover (See Cover Removal Note.)
2 | Screw (See Screw Installation Note.)
3 | Lower module

4. Install in the reverse order of removal.

## Cover Removal Note

1. Insert the SST into the service holes on the bottom surface of the lower module.

2. To remove the cover, push the SST in the direction shown by the arrow.

## Screw Installation Note

  Caution

  • If an undesignated screw is used, the inside of the upper module could be damaged. When installing the module, be sure to use a designated screw (red).