#
REAR A/C UNIT REMOVAL/INSTALLATION

BME07116187X201

1. Disconnect the negative battery cable.

2. Drain the engine coolant.

3. Evacuate the refrigerant from the system. (See REFRIGERANT CHARGING.)

4. Remove the right side trunk side trim.

5. Remove the rear heat duct No.4.

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise will occur. Always immediately plug open fittings after removing any refrigeration cycle parts to keep moisture or foreign material out of the cycle.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

8. Perform the refrigerant system performance test.

1 | Rear heater hose No.1 (See Heater Pipe and Hose Component Installation Note)
2 | Rear heater hose No.2 (See Heater Pipe and Hose Component Installation Note)
3 | Rear cooler pipe No.2 (See Refrigerant Lines Removal Note) (See Refrigerant Lines Installation Note)
4 | Connector
5 | Rear A/C unit