#
DTC TABLE [JA5A-EL]

BME050218901204

DTC No. | Condition | MIL | HOLD indicator light flashes | DC | *1Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0705 | Transaxle range (TR) switch circuit malfunction (power short circuit) | ON | YES | 2 | CCM | X | (See DTC P0705 [JA5A-EL])
P0706 | Transaxle range (TR) switch circuit malfunction (open/ground short circuit) | ON | YES | 2 | CCM | X | (See DTC P0706 [JA5A-EL])
P0711*2 | Transaxle fluid temperature (TFT) sensor malfunction (stuck) | ON | NO | 2 | CCM | X | (See DTC P0711 (ISRAELI SPECS.) [JA5A-EL])
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short circuit) | ON | YES | 2 | CCM | X | (See DTC P0712 [JA5A-EL])
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | ON | YES | 2 | CCM | X | (See DTC P0713 [JA5A-EL])
P0715 | Input/turbine speed sensor circuit malfunction | ON | YES | 2 | CCM | X | (See DTC P0715 [JA5A-EL])
P0720 | Vehicle speedometer sensor (VSS) circuit malfunction | ON | YES | 2 | CCM | X | (See DTC P0720 [JA5A-EL])
P0740*2 | Torque converter clutch (TCC) system malfunction | ON | NO | 2 | CCM | X | (See DTC P0740 (ISRAELI SPECS.) [JA5A-EL])
P0743 | Torque converter clutch (TCC) solenoid valve circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0743 [JA5A-EL])
P0748 | Pressure control solenoid circuit malfunction | OFF | YES | - | CCM | X | (See DTC P0748 [JA5A-EL])
P0751*2 | Shift solenoid A malfunction (stuck off) | ON | NO | 2 | CCM | X | (See DTC P0751 (ISRAELI SPECS.) [JA5A-EL])
P0752*2 | Shift solenoid A malfunction (stuck on) | ON | NO | 2 | CCM | X | (See DTC P0752 (ISRAELI SPECS.) [JA5A-EL])
P0753 | Shift solenoid A circuit malfunction (open/short) | ON | YES | 1 | CCM | X | (See DTC P0753 [JA5A-EL])
P0756*2 | Shift solenoid B malfunction (stuck off) | ON | NO | 2 | CCM | X | (See DTC P0756 (ISRAELI SPECS.) [JA5A-EL])
P0757*2 | Shift solenoid B malfunction (stuck on) | ON | NO | 2 | CCM | X | (See DTC P0757 (ISRAELI SPECS.) [JA5A-EL])
P0758 | Shift solenoid B circuit malfunction (open/short) | ON | YES | 1 | CCM | X | (See DTC P0758 [JA5A-EL])
P0761*2 | Shift solenoid C malfunction (stuck off) | ON | NO | 2 | CCM | X | (See DTC P0761 (ISRAELI SPECS.) [JA5A-EL])
P0762*2 | Shift solenoid C malfunction (stuck on) | ON | NO | 2 | CCM | X | (See DTC P0762 (ISRAELI SPECS.) [JA5A-EL])
P0763 | Shift solenoid C circuit malfunction (open/short) | ON | YES | 1 | CCM | X | (See DTC P0763 [JA5A-EL])
P0768 | Reduction timing solenoid valve circuit malfunction (open/short) | OFF | YES | - | CCM | X | (See DTC P0768 [JA5A-EL])
P0773 | Neutral shift solenoid valve circuit malfunction (open/short) | OFF | YES | - | CCM | X | (See DTC P0773 [JA5A-EL])
P0778 | 2-4 brake solenoid valve circuit malfunction (open/short) | OFF | YES | - | CCM | X | (See DTC P0778 [JA5A-EL])
P0791 | Intermediate sensor circuit malfunction (open/short) | ON | YES | 2 | CCM | X | (See DTC P0791 [JA5A-EL])
P0798 | High clutch solenoid valve circuit malfunction (open/short) | OFF | YES | - | CCM | X | (See DTC P0798 [JA5A-EL])
P1710 | GND return circuit malfunction | OFF | NO | - | Other | X | (See DTC P1710 [JA5A-EL])
U0073 | CAN BUS OFF | OFF | YES | 1 | CCM | X | (See DTC U0073 [JA5A-EL])
U0100 | TCM cannot receive any signals from PCM | ON | YES | 1 | CCM | X | (See DTC U0100 [JA5A-EL] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)) (See DTC U0100 [JA5A-EL] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)))

  *1 :
Indicates the applicable item in On-Board System Readiness Test defined by CARB.
  *2 :
Israeli specs.