#
DTC C1508 (92)

BME040243000216

DTC | C1508 (92) | TCS control
DETECTION CONDITION | • TCS control continues operation for 60 seconds or more.
POSSIBLE CAUSE | • System is normal. For protection of solenoid valves in the ABS/TCS HU/CM, or protection of the engine, sustained and continual control of TCS is inhibited.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear DTC from memory. (See Clearing DTCs Procedure) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above. • Is the same DTC present? | Yes | Replace ABS/TCS HU/CM, then go to next step.
No | Inspect intermittent concern using the same procedure as engine control system.
2 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to applicable DTC inspection.
No | Troubleshooting completed.