#
AIRFLOW MODE LINK REMOVAL/INSTALLATION

BME071161070W01

1. Remove the glove compartment.

2. Disconnect the airflow mode wire from the airflow mode link.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

  Note

  • Apply silicone grease or all-purpose grease to each link.

5. Adjust the airflow mode wire. (See FRONT CLIMATE CONTROL UNIT WIRE ADJUSTMENT.)

1 | Airflow mode crank
2 | Airflow mode link