#
FRONT DOOR DISASSEMBLY/ASSEMBLY

BME091158010202

  Caution

  • The automatic window return may not operate properly if the following is performed on the driver-side front door. (See DRIVER-SIDE POWER WINDOW MOTOR RESETTING.)

  - The power window motor is operated without the door glass properly installed.
  - The door glass is replaced.
  - The glass run channel is replaced.
  - The power window regulator is removed or installed. If a new power window regulator is installed, however, the power window motor does not require resetting.

1. Operate the front door glass so that the distance from the top of the front door glass at the rear end to the upper part of the front beltline molding is 185 mm {7.3 in}.

2. Disconnect the negative battery cable.

3. Remove the front door trim.

4. Disassemble in the order indicated in the table.

5. Assemble in the reverse order of disassembly.

1 | Inner handle
2 | Front door trim bracket
3 | Door screen
4 | Front door glass (See Front Door Glass Disassembly Note.)
5 | Front manual window regulator
6 | Front power window regulator
7 | Glass run channel
8 | Front door lock
9 | Outer handle (See Outer Handle Assembly Note.)
10 | Door key cylinder
11 | Door weatherstrip
12 | Door lower weatherstrip

## Front Door Glass Disassembly Note

1. Remove the front door glass installation bolts.

2. Slant the front door glass as shown, and remove the front door glass from the inside of the front door.

## Outer Handle Assembly Note

1. Connect the door key cylinder harness of outer handle as shown.