#
REAR CLIMATE CONTROL UNIT CONSTRUCTION

BME074061325T01
• A logic type rear climate control unit is used.
• The rear climate control unit adjusts the temperature and airflow of the rear A/C, and switches modes.
• Airflow adjustment of the rear climate control unit can be stopped by turning the rear main fan switch located on the dashboard to a position other than REAR position.

## With Rear A/C And Heater (Two Dial Type)

• A two-dial type, with mode and temperature, and fan control dials, has been adopted.
• A mode and temperature control dial integrating a mode dial and temperature control dial, has been adopted.
• Based on the mode and temperature control dial, cold air is blown in vent mode and hot air is blown in heat mode.

1 | Fan control dial
2 | Mode and temperature control dial
3 | HEAT, HOT
4 | VENT, COLD

## With Rear Heater (Two Dial Type)

• A two-dial type, with temperature and fan control dials, has been adopted.
• Temperature is adjusted using the temperature control dial.

1 | Fan control dial
2 | Temperature control dial