#
CRUISE ACTUATOR INSPECTION

BME012066310202

1. Disconnect the cruise actuator connector.

2. Measure the voltage, continuity and resistance at the cruise actuator terminals as indicated below.

  • If not as specified, inspect the parts listed under "Action."
  • If the parts and wiring harnesses are okay but the system still does not work properly, replace the cruise actuator.

## Terminal Voltage Table (Reference)

Terminal | Signal | Connected to | Test condition | Voltage (V) /Continuity | Action
--- | --- | --- | --- | --- | ---
A | Vehicle speed | Instrument cluster | 1. Ignition switch at ON position and cruise control main switch held at on. 2. Front tire rotating | Alternates below 1.0 and 5 | • Inspect METER 10 A fuse • Inspect instrument cluster (See INSTRUMENT CLUSTER INSPECTION) • Inspect related harness
B | Test | DLC | Under any condition: inspect for continuity to DLC terminal FSD | Yes | -
C | Brake switch on/off | Brake switch | Depress brake pedal | B+ | • Inspect brake switch (See BRAKE SWITCH INSPECTION) • Inspect related harness
Replace brake pedal | Below 1.0
D | Cruise control main switch input | Cruise control switch | Inspect for continuity to ground | Cruise control main switch held at on | Yes | • Inspect cruise control switch (See CRUISE CONTROL SWITCH INSPECTION) • Inspect related harness
Cruise control main switch off | No
E | O/D control | TCM | Ignition switch at ON position | B+ | • Inspect TCM (See PCM INSPECTION [FN4A-EL], TCM INSPECTION [JA5A-EL] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513), TCM INSPECTION [JA5A-EL] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)))
• Inspect related harness
F | Selector lever position | TR switch | Inspect for continuity to ground | Selector lever at N or P position | Yes | • Inspect TR switch (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL], TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL]) • Inspect starter • Inspect related harness
Other | No
G | Cruise set indicator light output | Cruise set indicator light | Ignition switch at ON position | B+ | • Inspect METER 10 A fuse • Inspect instrument cluster (See INSTRUMENT CLUSTER INSPECTION) • Inspect related harness
Ignition switch at LOCK position or ACC position | Below 1.0
H | - | - | - | - | -
I | Cruise actuator ground | GND | Under any condition: inspect for continuity to ground | Yes | • Inspect GND
J | Cruise control switch position | Cruise control switch | Inspect for resistance | SET/COAST switch held at on | Approx. 198 ohms | • Inspect cruise control switch (See CRUISE CONTROL SWITCH INSPECTION) • Inspect related harness
RESUME/ACCEL switch held at on | Approx. 68 ohms
CANCEL switch held at on | Approx. 418 ohms
K | Brake switch on/off | Brake switch 2 | Ignition switch at ON position | Depress brake pedal | Below 1.0 | • Inspect brake switch 2 (See BRAKE SWITCH INSPECTION) • Inspect related harness
Other | B+
L | IG1 | METER 10 A fuse | Ignition switch at ON position | B+ | • Inspect METER 10 A fuse • Inspect related harness
Ignition switch at LOCK position or ACC position | Below 1.0