#
SEDIMENTOR WATER DRAINING [MZR-CD (RF Turbo)]

BME011434802202

1. Disconnect the negative battery cable.

2. Complete the "BEFORE SERVICE PRECAUTION". (See BEFORE SERVICE PRECAUTION [MZR-CD (RF Turbo)].)

3. Loosen the drain plug located at the bottom of the fuel filter.

4. Pump the priming pump and drain the water.

5. After all the water has been drained, tighten the drain plug.

6. Complete the "AFTER SERVICE PRECAUTION". (See AFTER SERVICE PRECAUTION [MZR-CD (RF Turbo)].)

7. Reconnect the negative battery cable.