#
A/C COMPRESSOR REMOVAL/INSTALLATION

BME071161450201

1. Disconnect the negative battery cable.

2. Discharge the refrigerant from the system.

3. Remove the right side splash shield.

4. Loosen the drive belt and remove it.

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise will occur. Always immediately plug open fittings after removing any refrigeration cycle parts to keep moisture or foreign material out of the cycle.
  • Do not allow A/C compressor oil to spill. Operating the A/C compressor without sufficient A/C compressor oil can lead to abnormal noise and cause the A/C compressor to seize up.

5. Remove in the order indicated in the table.

1 | Cooler hose (HI) or front cooler pipe No.4 (See REFRIGERANT LINES REMOVAL/INSTALLATION)
2 | Cooler hose (LO) (See REFRIGERANT LINES REMOVAL/INSTALLATION)
3 | Connector
4 | A/C compressor

6. Install in the reverse order of removal.

7. Adjust the drive belt.

8. Perform the refrigerant system performance test.

## A/C Compressor Installation Note

1. Remove the following amount of compressor oil from the new A/C compressor when replacing the A/C compressor.

Compressor oil to be removed

  160 ml {160 cc, 5.40 fl oz} - compressor oil from old A/C compressor