#
TAPPET INSPECTION

A6E242412310E01

1. Measure the tappet hole inner diameter in X and Y directions at the two points (A and B) shown.

  Inner diameter:
  31.000-31.030 mm {1.2205-1.2216 in}

2. Measure the tappet body outer diameter in X and Y directions at the two points (A and B) shown.

  Outer diameter:
  30.970-30.980 mm {1.2193-1.2196 in}

3. Subtract the tappet body outer diameter from the tappet hole inner diameter.

  • If not as specified, replace the tappet or cylinder head.

  Clearance
  Standard:
  0.02-0.06 mm {0.0008-0.0023 in}
  Maximum:
  0.15 mm {0.006 in}