#
FRONT ANTENNA FEEDER INSPECTION

BME092066941W02

1. Remove the audio unit.

2. Remove the driver-side side panel.

3. Disconnect the connection between the front antenna and the rear antenna feeder.

4. Verify that there is no continuity between the front antenna feeder terminals A and B using an ohmmeter.

5. Inspect for continuity between the front antenna feeder terminals using an ohmmeter.

  • If not as specified, replace the instrument panel harness.