#
ROOF RAIL REMOVAL/INSTALLATION

BME091670600201

1. Remove the headliner.

2. Remove the shock absorbing pad.

3. To remove the right side roof rail, remove the rear cooler duct No.1.

4. Remove the nuts.

5. Pull the roof molding upward, then remove the double-sided adhesive tape from the roof.

6. Remove the screw, and remove the roof rail from the roof molding.

7. Install in the reverse order of removal.