#
CLUTCH SPECIFICATIONS

BME050000000T03

Item | Specifications
--- | ---
Manual transaxle type | G15M-R | A65M-R
Clutch control | Hydraulic
Clutch cover | Spring type | Diaphragm
Set load | (N {kgf, lbf}) | 6,000 {611, 1,350} | 6,550 {668, 1,472}
Clutch disc | Outer diameter | (mm {in}) | 215 {8.46} | 239 {9.41}
Inner diameter | (mm {in}) | 150 {5.91} | 160 {6.30}
Clutch pedal | Type |  | Suspended
Pedal ratio |  | 6.41
Full stroke (Reference value) | (mm {in}) | 148 {5.83}
Clutch master cylinder inner diameter | (mm {in}) | 15.87 {0.625}
Clutch release cylinder inner diameter | (mm {in}) | 19.05 {0.750}
Clutch fluid type |  | SAE J1703, FMVSS116 DOT-3 OR DOT-4