#
GLOW PLUG INSPECTION [MZR-CD (RF Turbo)]

BME011318601W02

  Note

  • Perform the following test only when directed.

1. Remove the glow plug lead. (See GLOW PLUG REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Inspect for continuity between the glow plug terminal and the cylinder head using an ohmmeter.

  • If there is no continuity, replace the glow plug.

Resistance

  Approx. 0.6 ohms [20°C {68°F}]

3. Install the glow plug lead.