#
MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY

BME074061010W01

1. Remove the A/C compressor. (See A/C COMPRESSOR REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

3. Assemble in the reverse order of disassembly.

4. Adjust the magnetic clutch clearance. (See MAGNETIC CLUTCH ADJUSTMENT.)

1 | Bolt (See Bolt Disassembly Note)
2 | Pressure plate
3 | Shim
4 | Snap ring
5 | A/C compressor pulley
6 | Snap ring
7 | Stator

## Bolt Disassembly Note

1. Remove the bolt using the SST.