#
SLIDE ADJUSTER DISASSEMBLY/ASSEMBLY

BME091357100W01

  Caution

  • When disassembling/assembling the slide adjuster, perform the work on a flat, level surface to prevent whine noise from the motors.

1. Remove the slide adjuster. (See FRONT SEAT DISASSEMBLY/ASSEMBLY.)

2. Disassemble in the order indicated in the table.

L.H.D.

.

1 | E-clip
2 | Front tilt motor
3 | E-clip
4 | Rear tilt motor
5 | Slide adjuster side plate
6 | Front lifter linkage

R.H.D.

.

1 | E-clip
2 | Front tilt motor
3 | E-clip
4 | Rear tilt motor
5 | Slide adjuster side plate
6 | Front lifter linkage

3. Assemble in the reverse order of disassembly.