#
JOINT SHAFT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME031325700W04

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor could cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Drain the transaxle oil.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

.

1 | Tie-rod end (See Tie-rod End Ball Joint Removal Note.)
2 | Lower arm ball joint (See Lower Arm Ball Joint Removal Note.)
3 | Stabilizer control link
4 | Drive shaft and axle assembly (See Drive Shaft and Axle Assembly Removal Note.)
5 | Joint shaft (See Joint Shaft Removal Note.) (See Joint Shaft Installation Note.)
6 | Clip (See Clip Installation Note.)