#
HVAC SPECIFICATIONS

BME070000000T10

Item | Specification
--- | ---
REFRIGERANT SYSTEM
Refrigerant | Type | R-134a
Regular amount (g {oz}) | Twin A/C | 800 {28.2}
Single A/C | 600 {21.2}
BASIC SYSTEM
Heating capacity (kW {kcal/h}) | Front | 5.580 {4,799}
Rear | 1.500 {1,290}
Cooling capacity (kW {kcal/h}) | Front | 5.800 {4,988}
Rear | 1.200 {1,032}
A/C compressor | Type | Swash plate
Discharge capacity (ml {cc, fl oz} /rev) | 177 {177, 5.98}
Max. allowable speed (rpm) | 6,000
Lubricating | Type | ND-OIL 8
Sealed volume (ml {cc, fl oz}) | 160 {160, 5.41}
Condenser | Type | Multiflow (sub-cooling system)
Radiated heat (kW {kcal/h}) | 8.88 {7,600}
Receiver/drier | Capacity (ml {cc, fl oz}) | 250 {250, 8.45}
Desiccant | XH-7
Expansion valve | Type | External pressure equalizer
Evaporator | Type | Drawn cup
CONTROL SYSTEM
Airflow volume (during heater operation) | Blower motor (m3/h) | Front | 380
Rear | 115
Electricity consumption (during heater operation) | Blower motor (W) | Front | 192
Rear | 100
Airflow volume (during air conditioner operation) | Blower motor (m3/h) | Front | 530
Rear | 180
Electricity consumption (during air conditioner operation) | Blower motor (W) | Front | 246
Rear | 100
Magnetic clutch (W) | 40
Magnetic clutch | Clearance (mm {in}) | 0.35-0.65 {0.014-0.025}
Blower motor | Fan type | Shroud fan
Temperature control | Reheat full air mix type
Refrigerant pressure switch | Type | Triple pressure
Operating pressure (MPa {kgf/cm2, psi}) |
Pressure relief valve | Operating pressure (MPa {kgf/cm2, psi}) | 3.44-4.13 {35.0-42.2, 498-600}