#
DTC 13

BME010266350215

DTC 13 | Cruise control switch (ground circuit)
--- | ---
DETECTION CONDITION | • Resistance detected between cruise actuator connector terminal J and ground is always approximately 0 ohm.
POSSIBLE CAUSE | • Cruise actuator malfunction

Diagnostic procedure

INSPECTION | ACTION
--- | ---
INSPECT DTC FOR OPERATION MODE • Was operation mode for DTCs 21 and 22 performed? | Yes | Perform operation mode for DTCs 21 and 22 on-board diagnostic again. Even if no malfunctions are detected in operation mode, if DTC 13 is indicated in condition detection mode on-board diagnostic, replace cruise actuator. (See CRUISE ACTUATOR REMOVAL/INSTALLATION)
No | Perform operation mode for DTCs 21 and 22.