#
REAR ANTENNA FEEDER No.1 REMOVAL/INSTALLATION

BME092066942201

1. Disconnect the negative battery cable.

2. Remove the passenger-side front side trim.

3. Remove the passenger-side A-pillar trim.

4. Remove the headliner.(See HEADLINER REMOVAL/INSTALLATION.)

5. Disconnect the connection between the front antenna feeder and the rear antenna feeder No.1.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

1 | Clip
2 | Bolt
3 | Rear antenna feeder No.1