#
HEADLINER REMOVAL/INSTALLATION

BME091768030W01

1. Disconnect the negative battery cable.

2. Turn the seaming welt and weatherstrip over.

3. Remove the A-pillar trims.

4. Remove the B-pillar upper trims.

5. Remove the C-pillar trims.

6. Remove the D-pillar trims.

7. Remove the map light. (See MAP LIGHT REMOVAL/INSTALLATION.)

8. Remove the interior light. (See INTERIOR LIGHT REMOVAL/INSTALLATION.)

9. Remove the screws, then remove the sunvisor and assist handle.

10. Fold hooks A up if equipped with a sliding sunroof.

11. Remove the fasteners.

12. Remove the headliner from the vehicle through the liftgate opening.

13. Install in the reverse order of removal.