#
GENERATOR CONSTRUCTION [L3]

BME011700000T04
• The voltage regulator has been eliminated, and generator control is carried out by the PCM.
• A Generator duct made of plastic and generator heat insulator made of iron have been adopted to protect the generator from the exhaust manifold heat.

1 | Generator
2 | Generator heat insulator
3 | Generator duct

.

1 | Stator coil
2 | Generator
3 | Power transistor
4 | PCM
5 | Ignition switch
6 | Generator warning light
7 | Battery