#
TRANSMITTER BATTERY REPLACEMENT

BME0914675DYW01

1. Insert a small flathead screwdriver into the slot and gently pry open the transmitter.

2. Remove the battery.

3. Install the new batteries with the negative side facing up.

Battery specification

  Lithium CR2025 × 1

  Note

  • The batteries will last about 2 years when used 10 times a day.

4. Align the front and back covers. (1)

5. Snap the transmitter shut. (2)