#
SUSPENSION TECHNICAL DATA

BME025001013201

## Suspension

Item | Specification
--- | ---
Front wheel alignment (Unloaded)*1 | Maximum steering angle | Inner | 37°06'±3°
Outer | 32°±3°
Total toe-in | (mm {in}) | 2±4 {0.08±0.16}
(°) | 0°11'±0° 22'
Camber angle*2 | -0°14'±1°
Caster angle*2 | 2°02'±1°
Kingpin angle (Reference value) | 11°11'
Rear wheel alignment (Unloaded)*1 | Total toe-in (Reference value) | (mm {in}) | 3±4 {0.12±0.16}
(°) | 0°17'±0°22'
Camber angle*2 (Reference value) | -1°±1°

  *1 :
Fuel tank is full. Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position. Adjust to the median when carrying out wheel alignment.
  *2 :
Difference between left and right must not exceed 1°30'.

## Wheels and Tires

### European (L.H.D. U.K.) specs

Item | Specification
--- | ---
Standard tire and wheel | Tire | Size | 205/65R15 94T | 215/60R16 95H
Air pressure (kPa {kgf/cm2, psi}) | Front | Up to 4 persons | 240 {2.5, 35}
More than 4 persons to full load | 250 {2.5, 36}
Rear | Up to 4 persons | 240 {2.5, 35}
More than 4 persons to full load | 290 {3.0, 42}
Remaining tread | Standard tire | (mm {in}) | 1.6 {0.06}
Snow tire | 50% of tread
Wheel | Size | 15 x 6 J | 15 x 6 JJ | 16 x 6 1/2J
Material | Aluminum alloy | Steel | Aluminum alloy
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Wheel and tire | Wheel and tire runout | (mm {in}) | Radial direction | 1.5 {0.06}
Lateral direction | 2.0 {0.08} | 2.5 {0.10} | 2.0 {0.08}
Wheel imbalance | (g {oz}) | Adhesive-type*1: 14 {0.49} max. Knock-type*2: 9 {0.32} max. | Knock-type*2: 9 {0.32} max. | Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max.
Temporary spare tire | Tire | Size | T135/90D 15 | T145/80D 16
Air pressure | (kPa {kgf/cm2, psi}) | 420 {4.2, 60}
Wheel | Size | 15 x 4T | 16 x 4T
Material | Steel
Offset | (mm {in}) | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

  *1 :
One balance weight: 160 g {5.64 oz} max. Do not use 3 or more balance weights.
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use 3 or more balance weights.

### Australian, General (L.H.D. R.H.D.) specs

Item | Specification
--- | ---
Standard tire and wheel | Tire | Size | 205/65R15 94H | 215/60R16 95H | 215/60R17 96H
Air pressure (kPa {kgf/cm2, psi}) | Front | 240 {2.5, 35}
Rear
Remaining tread | Standard tire | (mm {in}) | 1.6 {0.06}
Snow tire | 50% of tread
Wheel | Size | 15 x 6 J | 15 x 6 JJ | 16 x 6 1/2J | 17 x 7 J
Material | Aluminum alloy | Steel (Singapor specs.) | Aluminum alloy | Aluminum alloy (Singapor specs.)
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Wheel and tire | Wheel and tire runout | (mm {in}) | Radial direction | 1.5 {0.06}
Lateral direction | 2.0 {0.08} | 2.5 {0.10} | 2.0 {0.08}
Wheel imbalance | (g {oz}) | Adhesive-type*1: 14 {0.49} max. Knock-type*2: 9 {0.32} max. | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.38} max. Knock-type*2: 7 {0.25} max.
Temporary spare tire | Tire | Size | T135/90D 15 | T145/80D 16
Air pressure | (kPa {kgf/cm2, psi}) | 420 {4.2, 60}
Wheel | Size | 15 x 4T | 16 x 4T
Material | Steel
Offset | (mm {in}) | 35 {1.38} | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

  *1 :
One balance weight: 160 g {5.64 oz} max. Do not use 3 or more balance weights.
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use 3 or more balance weights.