#
CYLINDER HEAD (I) ASSEMBLY

A6E242402000E11

1. Assemble in the order indicated in the table.

1 | Water outlet case
2 | EGR pipe
3 | Valve seal (See Valve Seal Assembly Note)
4 | Valve
5 | Valve spring
6 | Upper valve spring seat
7 | Valve keeper (See Valve Keeper Assembly Note)
8 | Engine hanger

## Valve Seal Assembly Note

1. Press the valve seal onto the valve guide by hand.

2. Lightly tap the SST using a plastic hammer.

## Valve Keeper Assembly Note

1. Install the valve keeper using the SSTs.