#
THERMOSTAT REMOVAL/INSTALLATION [L3]

BME011215171201

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [L3].)

3. Remove the P/S oil pump without disconnecting the hose and the pipe.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [L3].)

1 | Bypass hose
2 | Lower radiator hose
3 | Thermostat