#
DTC B1317

BME070201038204

DTC B1317 | Input voltage high
DETECTION CONDITION | • Voltage detected at water heater unit terminals A is more than 16 V.
POSSIBLE CAUSE | • Short to power circuit between the generator and PCM • Generator malfunction • Battery malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT BATTERY VOLTAGE • Measure battery boltage. • Is voltage less than 16 V? | Yes | Go to next step.
No | Inspect charging system.
2 | INSPECT WATER HEATER UNIT • Clear the DTC. • Perform the KOEO Self Test. (See KOEO Self Test/Combustion Test.) • Is the same DTC present? | Yes | Replace the water heater unit. (See WATER HEATER UNIT REMOVAL/INSTALLATION)
No | Go to the next step.
3 | VERIFY AFTER REPAIR PROCEDURE • Perform the after repair procedure. (See After Repair Procedure.) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting.
No | Troubleshooting completed.